AlleSeiten

Summary Report | Date: Jun 12 2017
--- | ---

Rating of: ISO18571

Description: Examples from Annex A
Rating:

No. | Load Case | Rating | Weight
--- | --- | --- | ---
1 | Test 1_1 | ( 0.905) | 1.0
2 | Test 2_2 | ( 0.510) | 1.0
3 | Test 3_2 | ( 0.783) | 1.0
4 | Test 4_3 | ( 0.675) | 1.0
5 | Test 5_1 | ( 0.794) | 1.0

Total rating

( 0.733)

5.0

Load Case Report | Date: Jun 12 2017
--- | ---

Rating of: Test 1_1
Description: Acceleration 1
Rating:

No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.919) | 1.0
2 | Cae 2 | ( 0.883) | 1.0
3 | Cae 3 | ( 0.913) | 1.0

Total rating of load case 1:

( 0.905)

3.0

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 1
Description: Cae 1
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ACX0 | 0.919 | 1.0

Total rating of experiment 1:

( 0.919)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 1
Report of Signal 1 of Experiment 1: S1HEAD0000H3ACX0
Overall Rating: 0.919

Average of tests

annex_a_1_1_cae1

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.956 |  | 0.40
2 | Phase | 0.952 |  | 0.20
3 | Magnitude | 0.950 |  | 0.20
4 | Slope | 0.780 |  | 0.20
| Overall rating | 0.919 | Good | -

Parameters: | Evaluation Intervall: | 1.6 - 32.6
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 322.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 6.2
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 2
Description: Cae 2
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ACX0 | 0.883 | 1.0

Total rating of experiment 2:

( 0.883)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 2
Report of Signal 1 of Experiment 2: S1HEAD0000H3ACX0
Overall Rating: 0.883

Average of tests

annex_a_1_1_cae2

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.898 |  | 0.40
2 | Phase | 0.919 |  | 0.20
3 | Magnitude | 0.963 |  | 0.20
4 | Slope | 0.736 |  | 0.20
| Overall rating | 0.883 | Good | -

Parameters: | Evaluation Intervall: | 1.6 - 32.6
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 322.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 6.2
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 3
Description: Cae 3
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ACX0 | 0.913 | 1.0

Total rating of experiment 3:

( 0.913)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 3
Report of Signal 1 of Experiment 3: S1HEAD0000H3ACX0
Overall Rating: 0.913

Average of tests

annex_a_1_1_cae3

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.922 |  | 0.40
2 | Phase | 0.984 |  | 0.20
3 | Magnitude | 0.971 |  | 0.20
4 | Slope | 0.765 |  | 0.20
| Overall rating | 0.913 | Good | -

Parameters: | Evaluation Intervall: | 1.6 - 32.6
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 322.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 6.2
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jun 12 2017
--- | ---

Rating of: Test 2_2
Description: Angle 1
Rating:

No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.589) | 1.0
2 | Cae 2 | ( 0.360) | 1.0
3 | Cae 3 | ( 0.581) | 1.0

Total rating of load case 2:

( 0.510)

3.0

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 1
Description: Cae 1
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ANX0 | 0.589 | 1.0

Total rating of experiment 1:

( 0.589)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 1
Report of Signal 1 of Experiment 1: S1HEAD0000H3ANX0
Overall Rating: 0.589

Average of tests

annex_a_2_2_cae1

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.403 |  | 0.40
2 | Phase | 0.719 |  | 0.20
3 | Magnitude | 0.747 |  | 0.20
4 | Slope | 0.674 |  | 0.20
| Overall rating | 0.589 | Fair | -

Parameters: | Evaluation Intervall: | 5.1 - 147.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 0.284
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 28.5
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 2
Description: Cae 2
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ANX0 | 0.360 | 1.0

Total rating of experiment 2:

( 0.360)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 2
Report of Signal 1 of Experiment 2: S1HEAD0000H3ANX0
Overall Rating: 0.360

Average of tests

annex_a_2_2_cae2

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.287 |  | 0.40
2 | Phase | 0.905 |  | 0.20
3 | Magnitude | 0.094 |  | 0.20
4 | Slope | 0.226 |  | 0.20
| Overall rating | 0.360 | Poor | -

Parameters: | Evaluation Intervall: | 5.1 - 147.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 0.284
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 28.5
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 3
Description: Cae 3
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ANX0 | 0.581 | 1.0

Total rating of experiment 3:

( 0.581)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 3
Report of Signal 1 of Experiment 3: S1HEAD0000H3ANX0
Overall Rating: 0.581

Average of tests

annex_a_2_2_cae3

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.374 |  | 0.40
2 | Phase | 0.744 |  | 0.20
3 | Magnitude | 0.635 |  | 0.20
4 | Slope | 0.778 |  | 0.20
| Overall rating | 0.581 | Fair | -

Parameters: | Evaluation Intervall: | 5.1 - 147.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 0.284
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 28.5
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jun 12 2017
--- | ---

Rating of: Test 3_2
Description: Displacement 2
Rating:

No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.650) | 1.0
2 | Cae 2 | ( 0.863) | 1.0
3 | Cae 3 | ( 0.836) | 1.0

Total rating of load case 3:

( 0.783)

3.0

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 1
Description: Cae 1
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3DSX0 | 0.650 | 1.0

Total rating of experiment 1:

( 0.650)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 1
Report of Signal 1 of Experiment 1: S1HEAD0000H3DSX0
Overall Rating: 0.650

Average of tests

annex_a_3_2_cae1

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.469 |  | 0.40
2 | Phase | 0.807 |  | 0.20
3 | Magnitude | 0.679 |  | 0.20
4 | Slope | 0.826 |  | 0.20
| Overall rating | 0.650 | Fair | -

Parameters: | Evaluation Intervall: | 10.0 - 80.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 3.05e-005
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 14.1
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 2
Description: Cae 2
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3DSX0 | 0.863 | 1.0

Total rating of experiment 2:

( 0.863)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 2
Report of Signal 1 of Experiment 2: S1HEAD0000H3DSX0
Overall Rating: 0.863

Average of tests

annex_a_3_2_cae2

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.807 |  | 0.40
2 | Phase | 0.936 |  | 0.20
3 | Magnitude | 0.940 |  | 0.20
4 | Slope | 0.823 |  | 0.20
| Overall rating | 0.863 | Good | -

Parameters: | Evaluation Intervall: | 10.0 - 80.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 3.05e-005
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 14.1
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 3
Description: Cae 3
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3DSX0 | 0.836 | 1.0

Total rating of experiment 3:

( 0.836)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 3
Report of Signal 1 of Experiment 3: S1HEAD0000H3DSX0
Overall Rating: 0.836

Average of tests

annex_a_3_2_cae3

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.791 |  | 0.40
2 | Phase | 0.857 |  | 0.20
3 | Magnitude | 0.951 |  | 0.20
4 | Slope | 0.787 |  | 0.20
| Overall rating | 0.836 | Good | -

Parameters: | Evaluation Intervall: | 10.0 - 80.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 3.05e-005
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 14.1
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jun 12 2017
--- | ---

Rating of: Test 4_3
Description: Force 3
Rating:

No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.712) | 1.0
2 | Cae 2 | ( 0.450) | 1.0
3 | Cae 3 | ( 0.863) | 1.0

Total rating of load case 4:

( 0.675)

3.0

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 1
Description: Cae 1
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3FOX0 | 0.712 | 1.0

Total rating of experiment 1:

( 0.712)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 1
Report of Signal 1 of Experiment 1: S1HEAD0000H3FOX0
Overall Rating: 0.712

Average of tests

annex_a_4_3_cae1

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.653 |  | 0.40
2 | Phase | 0.977 |  | 0.20
3 | Magnitude | 0.733 |  | 0.20
4 | Slope | 0.547 |  | 0.20
| Overall rating | 0.712 | Fair | -

Parameters: | Evaluation Intervall: | 4.3 - 90.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 784.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.3
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 2
Description: Cae 2
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3FOX0 | 0.450 | 1.0

Total rating of experiment 2:

( 0.450)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 2
Report of Signal 1 of Experiment 2: S1HEAD0000H3FOX0
Overall Rating: 0.450

Average of tests

annex_a_4_3_cae2

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.493 |  | 0.40
2 | Phase | 0.873 |  | 0.20
3 | Magnitude | 0.276 |  | 0.20
4 | Slope | 0.116 |  | 0.20
| Overall rating | 0.450 | Poor | -

Parameters: | Evaluation Intervall: | 4.3 - 90.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 784.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.3
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 3
Description: Cae 3
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3FOX0 | 0.863 | 1.0

Total rating of experiment 3:

( 0.863)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 3
Report of Signal 1 of Experiment 3: S1HEAD0000H3FOX0
Overall Rating: 0.863

Average of tests

annex_a_4_3_cae3

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.903 |  | 0.40
2 | Phase | 0.960 |  | 0.20
3 | Magnitude | 0.928 |  | 0.20
4 | Slope | 0.623 |  | 0.20
| Overall rating | 0.863 | Good | -

Parameters: | Evaluation Intervall: | 4.3 - 90.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 784.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.3
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jun 12 2017
--- | ---

Rating of: Test 5_1
Description: Moment 1
Rating:

No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.821) | 1.0
2 | Cae 2 | ( 0.755) | 1.0
3 | Cae 3 | ( 0.807) | 1.0

Total rating of load case 5:

( 0.794)

3.0

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 1
Description: Cae 1
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3MOX0 | 0.821 | 1.0

Total rating of experiment 1:

( 0.821)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 1
Report of Signal 1 of Experiment 1: S1HEAD0000H3MOX0
Overall Rating: 0.821

Average of tests

annex_a_5_1_cae1

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.740 |  | 0.40
2 | Phase | 0.978 |  | 0.20
3 | Magnitude | 0.908 |  | 0.20
4 | Slope | 0.738 |  | 0.20
| Overall rating | 0.821 | Good | -

Parameters: | Evaluation Intervall: | 7.3 - 30.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 180.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 4.6
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 2
Description: Cae 2
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3MOX0 | 0.755 | 1.0

Total rating of experiment 2:

( 0.755)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 2
Report of Signal 1 of Experiment 2: S1HEAD0000H3MOX0
Overall Rating: 0.755

Average of tests

annex_a_5_1_cae2

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.723 |  | 0.40
2 | Phase | 0.587 |  | 0.20
3 | Magnitude | 0.966 |  | 0.20
4 | Slope | 0.775 |  | 0.20
| Overall rating | 0.755 | Fair | -

Parameters: | Evaluation Intervall: | 7.3 - 30.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 180.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 4.6
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jun 12 2017
--- | ---

Report of Experiment: Cae 3
Description: Cae 3
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3MOX0 | 0.807 | 1.0

Total rating of experiment 3:

( 0.807)

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 3
Report of Signal 1 of Experiment 3: S1HEAD0000H3MOX0
Overall Rating: 0.807

Average of tests

annex_a_5_1_cae3

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.790 |  | 0.40
2 | Phase | 0.804 |  | 0.20
3 | Magnitude | 0.961 |  | 0.20
4 | Slope | 0.687 |  | 0.20
| Overall rating | 0.807 | Good | -

Parameters: | Evaluation Intervall: | 7.3 - 30.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 180.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 4.6
| Rating exponents (shape, size, phase): | 1, 1, 1