Load Case 3 Experiment 2 Signal 1

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Cae 2
Report of Signal 1 of Experiment 2: S1HEAD0000H3DSX0
Overall Rating: 0.863

Average of tests

annex_a_3_2_cae2

CAE cut and shifted

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Grade | Weight
1 | Corridor | 0.807 |  | 0.40
2 | Phase | 0.936 |  | 0.20
3 | Magnitude | 0.940 |  | 0.20
4 | Slope | 0.823 |  | 0.20
| Overall rating | 0.863 | Good | -

Parameters: | Evaluation Intervall: | 10.0 - 80.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 3.05e-005
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 14.1
| Rating exponents (shape, size, phase): | 1, 1, 1

|  | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---