AlleSeiten

Summary Report | Date: Jun 12 2017
--- | ---

Rating of: Droptest and CAE-Droptest

Description: CORA sample data set loadcase 02
Rating:

No. | Load Case | Rating | Weight
--- | --- | --- | ---
1 | Evaluation of CAE_Droptest_01 | 0.953 | 0.50
2 | Evaluation of CAE_Droptest_02 | 0.70 | 0.50

Total rating

0.827

1.0

Load Case Report | Date: Jun 12 2017
--- | ---

Rating of: Evaluation of CAE_Droptest_01
Description: Loadcase 02
Rating:

No. | Signals | Rating | Weight
--- | --- | --- | ---
1 | 00SENS010000ACZC | 0.929 | 0.50
2 | 00SENS010000VEZC | 0.977 | 0.50

Total rating of load case 1:

0.953

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Evaluation of CAE_Droptest_01
Report of Signal 1 of Load Case 1: 00SENS010000ACZC
Overall Rating: 0.929

droptest_01

Average of experiments

droptest_02

cross-correlation reference

cae_droptest_01

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.928 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.999 | 0.997 | 0.50
Size | 0.912 | 0.912 | 0.250
Phase shift | 0.2 | 0.815 | 0.250

0.930

0.50

3 | Combination of 1 and 2 | 0.929 | -

Parameters: | Evaluation Intervall: | 0.8 - 7.5
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 1494.545
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Evaluation of CAE_Droptest_01
Report of Signal 2 of Load Case 1: 00SENS010000VEZC
Overall Rating: 0.977

droptest_01

Average of experiments

droptest_02

cross-correlation reference

cae_droptest_01

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.995 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 1.0 | 0.999 | 0.50
Size | 0.918 | 0.918 | 0.250
Phase shift | 0.1 | 0.916 | 0.250

0.958

0.50

3 | Combination of 1 and 2 | 0.977 | -

Parameters: | Evaluation Intervall: | 1.4 - 6.7
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.045
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Load Case Report | Date: Jun 12 2017
--- | ---

Rating of: Evaluation of CAE_Droptest_02
Description: Loadcase 02
Rating:

No. | Signals | Rating | Weight
--- | --- | --- | ---
1 | 00SENS010000ACZC | 0.660 | 0.50
2 | 00SENS010000VEZC | 0.741 | 0.50

Total rating of load case 2:

0.70

1.0

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Evaluation of CAE_Droptest_02
Report of Signal 1 of Load Case 2: 00SENS010000ACZC
Overall Rating: 0.660

droptest_01

Average of experiments

droptest_02

cross-correlation reference

cae_droptest_02

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.546 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.993 | 0.968 | 0.50
Size | 0.618 | 0.618 | 0.250
Phase shift | 0.4 | 0.540 | 0.250

0.773

0.50

3 | Combination of 1 and 2 | 0.660 | -

Parameters: | Evaluation Intervall: | 0.8 - 7.5
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 1494.545
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Evaluation of CAE_Droptest_02
Report of Signal 2 of Load Case 2: 00SENS010000VEZC
Overall Rating: 0.741

droptest_01

Average of experiments

droptest_02

cross-correlation reference

cae_droptest_02

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.644 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.999 | 0.997 | 0.50
Size | 0.614 | 0.614 | 0.250
Phase shift | 0.2 | 0.741 | 0.250

0.838

0.50

3 | Combination of 1 and 2 | 0.741 | -

Parameters: | Evaluation Intervall: | 1.4 - 6.7
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.045
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.6
| Rating exponents (shape, size, phase): | 10, 1, 1