Load Case 1 Experiment 2 Signal 12

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 12 of Experiment 2: S1SENS050000DSXC
Overall Rating: 0.675

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.574 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.986 | 0.930 | 0.50
Size | 0.816 | 0.816 | 0.250
Phase shift | 13.2 | 0.425 | 0.250

0.775

0.50

3 | Combination of 1 and 2 | 0.675 | -

Parameters: | Evaluation Intervall: | 14.0 - 194.2
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.022
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Previous Signal |  | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---