AlleSeiten

Summary Report | Date: Jun 21 2017
--- | ---

Rating of: Test and CAE

Description: CORA sample data set loadcase 01
Rating:

No. | Load Case | Rating | Weight
--- | --- | --- | ---
1 | Evaluation of CAE_01/02 | 0.657 | 1.0

Total rating

0.657

1.0

Load Case Report | Date: Jun 21 2017
--- | ---

Rating of: Evaluation of CAE_01/02
Description: Loadcase 01
Rating:

No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | CAE 1 | 0.651 | 0.50
2 | CAE 2 | 0.664 | 0.50

Total rating of load case 1:

0.657

1.0

Experiment Report | Date: Jun 21 2017
--- | ---

Report of Experiment: CAE 1
Description: Using ISO format 1.0
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1SENS010000DS0D | 0.658 | 0.083
2 | S1SENS020000FO0D | 0.958 | 0.083
3 | S1SENS030000ACXA | 0.822 | 0.083
4 | S1SENS030000ACYA | 0.389 | 0.083
5 | S1SENS030000ACZA | 0.796 | 0.083
6 | S1SENS040000FOXA | 0.877 | 0.083
7 | S1SENS040000FOYA | 0.445 | 0.083
8 | S1SENS040000FOZA | 0.826 | 0.083
9 | S1SENS040000MOXB | 0.263 | 0.083
10 | S1SENS040000MOYB | 0.668 | 0.083
11 | S1SENS040000MOZB | 0.335 | 0.083
12 | S1SENS050000DSXC | 0.777 | 0.083

Total rating of experiment 1:

0.651

1.0

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 1 of Experiment 1: S1SENS010000DS0D
Overall Rating: 0.658

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.481 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.961 | 0.823 | 0.50
Size | 0.711 | 0.711 | 0.250
Phase shift | 2.3 | 0.981 | 0.250

0.834

0.50

3 | Combination of 1 and 2 | 0.658 | -

Parameters: | Evaluation Intervall: | 10.1 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.089
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.9 - 22.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 2 of Experiment 1: S1SENS020000FO0D
Overall Rating: 0.958

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.934 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.997 | 0.984 | 0.50
Size | 0.959 | 0.959 | 0.250
Phase shift | -1.1 | 1.0 | 0.250

0.982

0.50

3 | Combination of 1 and 2 | 0.958 | -

Parameters: | Evaluation Intervall: | 9.9 - 169.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 3203.929
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 3 of Experiment 1: S1SENS030000ACXA
Overall Rating: 0.822

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.762 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.976 | 0.887 | 0.50
Size | 0.789 | 0.789 | 0.250
Phase shift | 2.5 | 0.968 | 0.250

0.883

0.50

3 | Combination of 1 and 2 | 0.822 | -

Parameters: | Evaluation Intervall: | 15.7 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 134.163
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 4 of Experiment 1: S1SENS030000ACYA
Overall Rating: 0.389

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.327 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.872 | 0.515 | 0.50
Size | 0.094 | 0.094 | 0.250
Phase shift | -8.4 | 0.677 | 0.250

0.450

0.50

3 | Combination of 1 and 2 | 0.389 | -

Parameters: | Evaluation Intervall: | 15.3 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 17.707
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 5 of Experiment 1: S1SENS030000ACZA
Overall Rating: 0.796

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.750 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.929 | 0.698 | 0.50
Size | 0.973 | 0.973 | 0.250
Phase shift | -1.0 | 1.0 | 0.250

0.842

0.50

3 | Combination of 1 and 2 | 0.796 | -

Parameters: | Evaluation Intervall: | 13.5 - 159.8
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 166.750
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 6 of Experiment 1: S1SENS040000FOXA
Overall Rating: 0.877

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.846 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.988 | 0.942 | 0.50
Size | 0.748 | 0.748 | 0.250
Phase shift | -0.4 | 1.0 | 0.250

0.908

0.50

3 | Combination of 1 and 2 | 0.877 | -

Parameters: | Evaluation Intervall: | 15.8 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 513.896
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 7 of Experiment 1: S1SENS040000FOYA
Overall Rating: 0.445

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.318 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.937 | 0.725 | 0.50
Size | 0.178 | 0.178 | 0.250
Phase shift | -7.6 | 0.660 | 0.250

0.572

0.50

3 | Combination of 1 and 2 | 0.445 | -

Parameters: | Evaluation Intervall: | 18.5 - 178.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 109.973
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 8 of Experiment 1: S1SENS040000FOZA
Overall Rating: 0.826

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.761 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.955 | 0.795 | 0.50
Size | 0.978 | 0.978 | 0.250
Phase shift | -1.4 | 1.0 | 0.250

0.892

0.50

3 | Combination of 1 and 2 | 0.826 | -

Parameters: | Evaluation Intervall: | 13.7 - 160.3
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 750.624
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 9 of Experiment 1: S1SENS040000MOXB
Overall Rating: 0.263

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.167 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.762 | 0.282 | 0.50
Size | 0.098 | 0.098 | 0.250
Phase shift | -6.2 | 0.777 | 0.250

0.360

0.50

3 | Combination of 1 and 2 | 0.263 | -

Parameters: | Evaluation Intervall: | 20.6 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.047
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.5
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 10 of Experiment 1: S1SENS040000MOYB
Overall Rating: 0.668

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.643 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.851 | 0.462 | 0.50
Size | 0.922 | 0.922 | 0.250
Phase shift | 3.3 | 0.928 | 0.250

0.693

0.50

3 | Combination of 1 and 2 | 0.668 | -

Parameters: | Evaluation Intervall: | 16.4 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 38.820
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.0
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 11 of Experiment 1: S1SENS040000MOZB
Overall Rating: 0.335

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.364 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.706 | 0.204 | 0.50
Size | 0.450 | 0.450 | 0.250
Phase shift | -14.6 | 0.370 | 0.250

0.307

0.50

3 | Combination of 1 and 2 | 0.335 | -

Parameters: | Evaluation Intervall: | 15.9 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 2.871
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 12 of Experiment 1: S1SENS050000DSXC
Overall Rating: 0.777

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.643 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.991 | 0.957 | 0.50
Size | 0.731 | 0.731 | 0.250
Phase shift | 1.9 | 0.995 | 0.250

0.910

0.50

3 | Combination of 1 and 2 | 0.777 | -

Parameters: | Evaluation Intervall: | 14.0 - 194.2
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.022
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Experiment Report | Date: Jun 21 2017
--- | ---

Report of Experiment: CAE 2
Description: Using XYData format
Rating:

No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1SENS010000DS0D | 0.752 | 0.083
2 | S1SENS020000FO0D | 0.914 | 0.083
3 | S1SENS030000ACXA | 0.802 | 0.083
4 | S1SENS030000ACYA | 0.295 | 0.083
5 | S1SENS030000ACZA | 0.858 | 0.083
6 | S1SENS040000FOXA | 0.891 | 0.083
7 | S1SENS040000FOYA | 0.555 | 0.083
8 | S1SENS040000FOZA | 0.869 | 0.083
9 | S1SENS040000MOXB | 0.262 | 0.083
10 | S1SENS040000MOYB | 0.763 | 0.083
11 | S1SENS040000MOZB | 0.329 | 0.083
12 | S1SENS050000DSXC | 0.675 | 0.083

Total rating of experiment 2:

0.664

1.0

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 1 of Experiment 2: S1SENS010000DS0D
Overall Rating: 0.752

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.599 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.979 | 0.899 | 0.50
Size | 0.824 | 0.824 | 0.250
Phase shift | 1.5 | 1.0 | 0.250

0.905

0.50

3 | Combination of 1 and 2 | 0.752 | -

Parameters: | Evaluation Intervall: | 10.1 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.089
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.9 - 22.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 2 of Experiment 2: S1SENS020000FO0D
Overall Rating: 0.914

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.872 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.991 | 0.954 | 0.50
Size | 0.917 | 0.917 | 0.250
Phase shift | 0.6 | 1.0 | 0.250

0.956

0.50

3 | Combination of 1 and 2 | 0.914 | -

Parameters: | Evaluation Intervall: | 9.9 - 169.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 3203.929
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 3 of Experiment 2: S1SENS030000ACXA
Overall Rating: 0.802

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.762 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.981 | 0.910 | 0.50
Size | 0.608 | 0.608 | 0.250
Phase shift | 3.1 | 0.938 | 0.250

0.841

0.50

3 | Combination of 1 and 2 | 0.802 | -

Parameters: | Evaluation Intervall: | 15.7 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 134.163
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 4 of Experiment 2: S1SENS030000ACYA
Overall Rating: 0.295

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.340 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.738 | 0.246 | 0.50
Size | 0.165 | 0.165 | 0.250
Phase shift | -15.2 | 0.342 | 0.250

0.250

0.50

3 | Combination of 1 and 2 | 0.295 | -

Parameters: | Evaluation Intervall: | 15.3 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 17.707
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 5 of Experiment 2: S1SENS030000ACZA
Overall Rating: 0.858

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.793 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.975 | 0.884 | 0.50
Size | 0.927 | 0.927 | 0.250
Phase shift | -0.4 | 1.0 | 0.250

0.924

0.50

3 | Combination of 1 and 2 | 0.858 | -

Parameters: | Evaluation Intervall: | 13.5 - 159.8
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 166.750
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 6 of Experiment 2: S1SENS040000FOXA
Overall Rating: 0.891

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.830 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.985 | 0.926 | 0.50
Size | 0.954 | 0.954 | 0.250
Phase shift | 0.6 | 1.0 | 0.250

0.951

0.50

3 | Combination of 1 and 2 | 0.891 | -

Parameters: | Evaluation Intervall: | 15.8 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 513.896
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 7 of Experiment 2: S1SENS040000FOYA
Overall Rating: 0.555

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.536 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.922 | 0.673 | 0.50
Size | 0.495 | 0.495 | 0.250
Phase shift | -11.3 | 0.450 | 0.250

0.573

0.50

3 | Combination of 1 and 2 | 0.555 | -

Parameters: | Evaluation Intervall: | 18.5 - 178.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 109.973
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 8 of Experiment 2: S1SENS040000FOZA
Overall Rating: 0.869

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.821 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.976 | 0.886 | 0.50
Size | 0.893 | 0.893 | 0.250
Phase shift | -0.8 | 1.0 | 0.250

0.916

0.50

3 | Combination of 1 and 2 | 0.869 | -

Parameters: | Evaluation Intervall: | 13.7 - 160.3
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 750.624
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 9 of Experiment 2: S1SENS040000MOXB
Overall Rating: 0.262

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.281 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.666 | 0.161 | 0.50
Size | 0.272 | 0.272 | 0.250
Phase shift | -14.0 | 0.381 | 0.250

0.244

0.50

3 | Combination of 1 and 2 | 0.262 | -

Parameters: | Evaluation Intervall: | 20.6 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.047
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.5
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 10 of Experiment 2: S1SENS040000MOYB
Overall Rating: 0.763

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.753 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.949 | 0.774 | 0.50
Size | 0.613 | 0.613 | 0.250
Phase shift | -3.2 | 0.932 | 0.250

0.773

0.50

3 | Combination of 1 and 2 | 0.763 | -

Parameters: | Evaluation Intervall: | 16.4 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 38.820
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.0
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 11 of Experiment 2: S1SENS040000MOZB
Overall Rating: 0.329

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.375 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.257 | 0.010 | 0.50
Size | 0.803 | 0.803 | 0.250
Phase shift | -15.8 | 0.310 | 0.250

0.283

0.50

3 | Combination of 1 and 2 | 0.329 | -

Parameters: | Evaluation Intervall: | 15.9 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 2.871
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 2
Report of Signal 12 of Experiment 2: S1SENS050000DSXC
Overall Rating: 0.675

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_02

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.574 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.986 | 0.930 | 0.50
Size | 0.816 | 0.816 | 0.250
Phase shift | 13.2 | 0.425 | 0.250

0.775

0.50

3 | Combination of 1 and 2 | 0.675 | -

Parameters: | Evaluation Intervall: | 14.0 - 194.2
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.022
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.6
| Rating exponents (shape, size, phase): | 10, 1, 1