Load Case 2 Signal 2

Signal Report | Date: Jun 12 2017
--- | ---

Rating of: Evaluation of CAE_Droptest_02
Report of Signal 2 of Load Case 2: 00SENS010000VEZC
Overall Rating: 0.741

droptest_01

Average of experiments

droptest_02

cross-correlation reference

cae_droptest_02

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.644 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.999 | 0.997 | 0.50
Size | 0.614 | 0.614 | 0.250
Phase shift | 0.2 | 0.741 | 0.250

0.838

0.50

3 | Combination of 1 and 2 | 0.741 | -

Parameters: | Evaluation Intervall: | 1.4 - 6.7
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.045
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Previous Signal |  | Up to Loadcase | Up to Summary
--- | --- | --- | ---