Load Case 1 Experiment 1 Signal 5

Signal Report | Date: Jun 21 2017
--- | ---

Rating of: CAE 1
Report of Signal 5 of Experiment 1: S1SENS030000ACZA
Overall Rating: 0.796

test_01

Average of experiments

test_02

cross-correlation reference

test_03

cae_01

test_04

Limits Outer corridor

Limits inner corridor

Method | Name | Rating | Weight
1 | Corridor Method | 0.750 | 0.50

2

Correlation Method |  |  |

| Value | Rating | Weight

Cross correlation function | 0.929 | 0.698 | 0.50
Size | 0.973 | 0.973 | 0.250
Phase shift | -1.0 | 1.0 | 0.250

0.842

0.50

3 | Combination of 1 and 2 | 0.796 | -

Parameters: | Evaluation Intervall: | 13.5 - 159.8
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 166.750
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Previous Signal | Next Signal | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---