Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_Droptest_01 Report of Signal 1 of Load Case 1: 00SENS010000ACZC Overall Rating: 0.9292
| droptest_01 |  | Average of experiments
| droptest_02 |  | cross-correlation reference
|  |  | cae_droptest_01
|  |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.9281 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9994 | 0.9968 | 0.50
Size | 0.9117 | 0.9117 | 0.250
Phase shift | 0.2 | 0.8154 | 0.250
| 0.9302 | 0.50
3 | Combination of 1 and 2 | 0.9292 | -
Parameters: | Evaluation Intervall: | 0.8 - 7.5
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 1494.5445
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.8
| Rating exponents (shape, size, phase): | 10, 1, 1
| Next Signal | Up to Loadcase | Up to Summary
--- | --- | --- | ---