Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 4 of Experiment 2: S1SENS030000ACYA Overall Rating: 0.2946
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.3396 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.7380 | 0.2455 | 0.50
Size | 0.1653 | 0.1653 | 0.250
Phase shift | -15.2 | 0.3424 | 0.250
| 0.2497 | 0.50
3 | Combination of 1 and 2 | 0.2946 | -
Parameters: | Evaluation Intervall: | 15.3 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 17.7066
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.2
| Rating exponents (shape, size, phase): | 10, 1, 1
Previous Signal | Next Signal | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---