Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 3 Report of Signal 1 of Experiment 3: S1HEAD0000H3ANX0 Overall Rating: 0.5831
| Average of tests
| annex_a_2_2_cae3
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.3737 |  | 0.40
2 | Phase | 0.7446 |  | 0.20
3 | Magnitude | 0.6422 |  | 0.20
4 | Slope | 0.7815 |  | 0.20
| Overall rating | 0.5831 | Fair | -
Parameters: | Evaluation Intervall: | 5.1 - 147.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 0.2840
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 28.5
| Rating exponents (shape, size, phase): | 1, 1, 1
|  | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---