Summary Report | Date: Jan 12 2026
--- | ---
Rating of: Droptest and CAE-Droptest
Description: CORA sample data set loadcase 02 Rating:
No. | Load Case | Rating | Weight
--- | --- | --- | ---
1 | Evaluation of CAE_Droptest_01 | 0.9529 | 0.50
2 | Evaluation of CAE_Droptest_02 | 0.7002 | 0.50
| Total rating | 0.8266 | 1.0

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_Droptest_01 Description: Loadcase 02 Rating:
No. | Signals | Rating | Weight
--- | --- | --- | ---
1 | 00SENS010000ACZC | 0.9292 | 0.50
2 | 00SENS010000VEZC | 0.9766 | 0.50
| Total rating of load case 1: | 0.9529 | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_Droptest_01 Report of Signal 1 of Load Case 1: 00SENS010000ACZC Overall Rating: 0.9292
| droptest_01 |  | Average of experiments
| droptest_02 |  | cross-correlation reference
|  |  | cae_droptest_01
|  |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.9281 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9994 | 0.9968 | 0.50
Size | 0.9117 | 0.9117 | 0.250
Phase shift | 0.2 | 0.8154 | 0.250
| 0.9302 | 0.50
3 | Combination of 1 and 2 | 0.9292 | -
Parameters: | Evaluation Intervall: | 0.8 - 7.5
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 1494.5445
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_Droptest_01 Report of Signal 2 of Load Case 1: 00SENS010000VEZC Overall Rating: 0.9766
| droptest_01 |  | Average of experiments
| droptest_02 |  | cross-correlation reference
|  |  | cae_droptest_01
|  |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.9949 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9999 | 0.9995 | 0.50
Size | 0.9182 | 0.9182 | 0.250
Phase shift | 0.1 | 0.9161 | 0.250
| 0.9583 | 0.50
3 | Combination of 1 and 2 | 0.9766 | -
Parameters: | Evaluation Intervall: | 1.4 - 6.7
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.0445
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_Droptest_02 Description: Loadcase 02 Rating:
No. | Signals | Rating | Weight
--- | --- | --- | ---
1 | 00SENS010000ACZC | 0.6599 | 0.50
2 | 00SENS010000VEZC | 0.7406 | 0.50
| Total rating of load case 2: | 0.7002 | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_Droptest_02 Report of Signal 1 of Load Case 2: 00SENS010000ACZC Overall Rating: 0.6599
| droptest_01 |  | Average of experiments
| droptest_02 |  | cross-correlation reference
|  |  | cae_droptest_02
|  |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.5465 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9934 | 0.9675 | 0.50
Size | 0.6181 | 0.6181 | 0.250
Phase shift | 0.4 | 0.5399 | 0.250
| 0.7733 | 0.50
3 | Combination of 1 and 2 | 0.6599 | -
Parameters: | Evaluation Intervall: | 0.8 - 7.5
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 1494.5447
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_Droptest_02 Report of Signal 2 of Load Case 2: 00SENS010000VEZC Overall Rating: 0.7406
| droptest_01 |  | Average of experiments
| droptest_02 |  | cross-correlation reference
|  |  | cae_droptest_02
|  |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.6437 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9995 | 0.9973 | 0.50
Size | 0.6142 | 0.6142 | 0.250
Phase shift | 0.2 | 0.7413 | 0.250
| 0.8375 | 0.50
3 | Combination of 1 and 2 | 0.7406 | -
Parameters: | Evaluation Intervall: | 1.4 - 6.7
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.0445
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 0.1 - 0.6
| Rating exponents (shape, size, phase): | 10, 1, 1