Summary Report | Date: Jan 12 2026
--- | ---
Rating of: ISO18571
Description: Examples from Annex A Rating:
No. | Load Case | Rating | Weight
--- | --- | --- | ---
1 | Test 1_1 | ( 0.9046) | 1.0
2 | Test 2_2 | ( 0.5739) | 1.0
3 | Test 3_2 | ( 0.7839) | 1.0
4 | Test 4_3 | ( 0.6816) | 1.0
5 | Test 5_1 | ( 0.7945) | 1.0
| Total rating | ( 0.7477) | 5.0

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Test 1_1 Description: Acceleration 1 Rating:
No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.9169) | 1.0
2 | Cae 2 | ( 0.8848) | 1.0
3 | Cae 3 | ( 0.9122) | 1.0
| Total rating of load case 1: | ( 0.9046) | 3.0

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 1 Description: Cae 1 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ACX0 | 0.9169 | 1.0
| Total rating of experiment 1: | ( 0.9169) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 1 Report of Signal 1 of Experiment 1: S1HEAD0000H3ACX0 Overall Rating: 0.9169
| Average of tests
| annex_a_1_1_cae1
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.9560 |  | 0.40
2 | Phase | 0.9518 |  | 0.20
3 | Magnitude | 0.9524 |  | 0.20
4 | Slope | 0.7683 |  | 0.20
| Overall rating | 0.9169 | Good | -
Parameters: | Evaluation Intervall: | 1.6 - 32.6
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 322.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 6.2
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 2 Description: Cae 2 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ACX0 | 0.8848 | 1.0
| Total rating of experiment 2: | ( 0.8848) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 2 Report of Signal 1 of Experiment 2: S1HEAD0000H3ACX0 Overall Rating: 0.8848
| Average of tests
| annex_a_1_1_cae2
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.8977 |  | 0.40
2 | Phase | 0.9196 |  | 0.20
3 | Magnitude | 0.9640 |  | 0.20
4 | Slope | 0.7449 |  | 0.20
| Overall rating | 0.8848 | Good | -
Parameters: | Evaluation Intervall: | 1.6 - 32.6
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 322.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 6.2
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 3 Description: Cae 3 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ACX0 | 0.9122 | 1.0
| Total rating of experiment 3: | ( 0.9122) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 3 Report of Signal 1 of Experiment 3: S1HEAD0000H3ACX0 Overall Rating: 0.9122
| Average of tests
| annex_a_1_1_cae3
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.9225 |  | 0.40
2 | Phase | 0.9839 |  | 0.20
3 | Magnitude | 0.9716 |  | 0.20
4 | Slope | 0.7606 |  | 0.20
| Overall rating | 0.9122 | Good | -
Parameters: | Evaluation Intervall: | 1.6 - 32.6
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 322.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 6.2
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Test 2_2 Description: Angle 1 Rating:
No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.5910) | 1.0
2 | Cae 2 | ( 0.5475) | 1.0
3 | Cae 3 | ( 0.5831) | 1.0
| Total rating of load case 2: | ( 0.5739) | 3.0

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 1 Description: Cae 1 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ANX0 | 0.5910 | 1.0
| Total rating of experiment 1: | ( 0.5910) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 1 Report of Signal 1 of Experiment 1: S1HEAD0000H3ANX0 Overall Rating: 0.5910
| Average of tests
| annex_a_2_2_cae1
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.4033 |  | 0.40
2 | Phase | 0.7201 |  | 0.20
3 | Magnitude | 0.7595 |  | 0.20
4 | Slope | 0.6688 |  | 0.20
| Overall rating | 0.5910 | Fair | -
Parameters: | Evaluation Intervall: | 5.1 - 147.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 0.2840
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 28.5
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 2 Description: Cae 2 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ANX0 | 0.5475 | 1.0
| Total rating of experiment 2: | ( 0.5475) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 2 Report of Signal 1 of Experiment 2: S1HEAD0000H3ANX0 Overall Rating: 0.5475
| Average of tests
| annex_a_2_2_cae2
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.4123 |  | 0.40
2 | Phase | 0.90 |  | 0.20
3 | Magnitude | 0.5957 |  | 0.20
4 | Slope | 0.4170 |  | 0.20
| Overall rating | 0.5475 | Poor | -
Parameters: | Evaluation Intervall: | 5.1 - 90.0
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 0.2840
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.0
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 3 Description: Cae 3 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3ANX0 | 0.5831 | 1.0
| Total rating of experiment 3: | ( 0.5831) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 3 Report of Signal 1 of Experiment 3: S1HEAD0000H3ANX0 Overall Rating: 0.5831
| Average of tests
| annex_a_2_2_cae3
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.3737 |  | 0.40
2 | Phase | 0.7446 |  | 0.20
3 | Magnitude | 0.6422 |  | 0.20
4 | Slope | 0.7815 |  | 0.20
| Overall rating | 0.5831 | Fair | -
Parameters: | Evaluation Intervall: | 5.1 - 147.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 0.2840
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 28.5
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Test 3_2 Description: Displacement 2 Rating:
No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.6512) | 1.0
2 | Cae 2 | ( 0.8635) | 1.0
3 | Cae 3 | ( 0.8370) | 1.0
| Total rating of load case 3: | ( 0.7839) | 3.0

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 1 Description: Cae 1 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3DSX0 | 0.6512 | 1.0
| Total rating of experiment 1: | ( 0.6512) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 1 Report of Signal 1 of Experiment 1: S1HEAD0000H3DSX0 Overall Rating: 0.6512
| Average of tests
| annex_a_3_2_cae1
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.4691 |  | 0.40
2 | Phase | 0.8085 |  | 0.20
3 | Magnitude | 0.6785 |  | 0.20
4 | Slope | 0.8308 |  | 0.20
| Overall rating | 0.6512 | Fair | -
Parameters: | Evaluation Intervall: | 10.0 - 80.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 3.05e-05
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 14.1
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 2 Description: Cae 2 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3DSX0 | 0.8635 | 1.0
| Total rating of experiment 2: | ( 0.8635) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 2 Report of Signal 1 of Experiment 2: S1HEAD0000H3DSX0 Overall Rating: 0.8635
| Average of tests
| annex_a_3_2_cae2
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.8074 |  | 0.40
2 | Phase | 0.9362 |  | 0.20
3 | Magnitude | 0.9423 |  | 0.20
4 | Slope | 0.8242 |  | 0.20
| Overall rating | 0.8635 | Good | -
Parameters: | Evaluation Intervall: | 10.0 - 80.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 3.05e-05
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 14.1
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 3 Description: Cae 3 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3DSX0 | 0.8370 | 1.0
| Total rating of experiment 3: | ( 0.8370) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 3 Report of Signal 1 of Experiment 3: S1HEAD0000H3DSX0 Overall Rating: 0.8370
| Average of tests
| annex_a_3_2_cae3
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.7915 |  | 0.40
2 | Phase | 0.8582 |  | 0.20
3 | Magnitude | 0.9552 |  | 0.20
4 | Slope | 0.7889 |  | 0.20
| Overall rating | 0.8370 | Good | -
Parameters: | Evaluation Intervall: | 10.0 - 80.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 3.05e-05
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 14.1
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Test 4_3 Description: Force 3 Rating:
No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.7125) | 1.0
2 | Cae 2 | ( 0.4682) | 1.0
3 | Cae 3 | ( 0.8640) | 1.0
| Total rating of load case 4: | ( 0.6816) | 3.0

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 1 Description: Cae 1 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3FOX0 | 0.7125 | 1.0
| Total rating of experiment 1: | ( 0.7125) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 1 Report of Signal 1 of Experiment 1: S1HEAD0000H3FOX0 Overall Rating: 0.7125
| Average of tests
| annex_a_4_3_cae1
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.6526 |  | 0.40
2 | Phase | 0.9769 |  | 0.20
3 | Magnitude | 0.7375 |  | 0.20
4 | Slope | 0.5426 |  | 0.20
| Overall rating | 0.7125 | Fair | -
Parameters: | Evaluation Intervall: | 4.3 - 90.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 784.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.3
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 2 Description: Cae 2 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3FOX0 | 0.4682 | 1.0
| Total rating of experiment 2: | ( 0.4682) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 2 Report of Signal 1 of Experiment 2: S1HEAD0000H3FOX0 Overall Rating: 0.4682
| Average of tests
| annex_a_4_3_cae2
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.4925 |  | 0.40
2 | Phase | 0.8731 |  | 0.20
3 | Magnitude | 0.3654 |  | 0.20
4 | Slope | 0.1172 |  | 0.20
| Overall rating | 0.4682 | Poor | -
Parameters: | Evaluation Intervall: | 4.3 - 90.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 784.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.3
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 3 Description: Cae 3 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3FOX0 | 0.8640 | 1.0
| Total rating of experiment 3: | ( 0.8640) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 3 Report of Signal 1 of Experiment 3: S1HEAD0000H3FOX0 Overall Rating: 0.8640
| Average of tests
| annex_a_4_3_cae3
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.9032 |  | 0.40
2 | Phase | 0.9596 |  | 0.20
3 | Magnitude | 0.9286 |  | 0.20
4 | Slope | 0.6256 |  | 0.20
| Overall rating | 0.8640 | Good | -
Parameters: | Evaluation Intervall: | 4.3 - 90.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 784.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.3
| Rating exponents (shape, size, phase): | 1, 1, 1

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Test 5_1 Description: Moment 1 Rating:
No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | Cae 1 | ( 0.8203) | 1.0
2 | Cae 2 | ( 0.7549) | 1.0
3 | Cae 3 | ( 0.8084) | 1.0
| Total rating of load case 5: | ( 0.7945) | 3.0

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 1 Description: Cae 1 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3MOX0 | 0.8203 | 1.0
| Total rating of experiment 1: | ( 0.8203) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 1 Report of Signal 1 of Experiment 1: S1HEAD0000H3MOX0 Overall Rating: 0.8203
| Average of tests
| annex_a_5_1_cae1
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.7402 |  | 0.40
2 | Phase | 0.9784 |  | 0.20
3 | Magnitude | 0.9099 |  | 0.20
4 | Slope | 0.7329 |  | 0.20
| Overall rating | 0.8203 | Good | -
Parameters: | Evaluation Intervall: | 7.3 - 30.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 180.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 4.6
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 2 Description: Cae 2 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3MOX0 | 0.7549 | 1.0
| Total rating of experiment 2: | ( 0.7549) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 2 Report of Signal 1 of Experiment 2: S1HEAD0000H3MOX0 Overall Rating: 0.7549
| Average of tests
| annex_a_5_1_cae2
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.7233 |  | 0.40
2 | Phase | 0.5905 |  | 0.20
3 | Magnitude | 0.9668 |  | 0.20
4 | Slope | 0.7703 |  | 0.20
| Overall rating | 0.7549 | Fair | -
Parameters: | Evaluation Intervall: | 7.3 - 30.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 180.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 4.6
| Rating exponents (shape, size, phase): | 1, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: Cae 3 Description: Cae 3 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1HEAD0000H3MOX0 | 0.8084 | 1.0
| Total rating of experiment 3: | ( 0.8084) | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 3 Report of Signal 1 of Experiment 3: S1HEAD0000H3MOX0 Overall Rating: 0.8084
| Average of tests
| annex_a_5_1_cae3
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.7901 |  | 0.40
2 | Phase | 0.8060 |  | 0.20
3 | Magnitude | 0.9618 |  | 0.20
4 | Slope | 0.6939 |  | 0.20
| Overall rating | 0.8084 | Good | -
Parameters: | Evaluation Intervall: | 7.3 - 30.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 180.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 4.6
| Rating exponents (shape, size, phase): | 1, 1, 1