Summary Report | Date: Jan 12 2026
--- | ---
Rating of: Test and CAE
Description: CORA sample data set loadcase 01 Rating:
No. | Load Case | Rating | Weight
--- | --- | --- | ---
1 | Evaluation of CAE_01/02 | 0.6574 | 1.0
| Total rating | 0.6574 | 1.0

Load Case Report | Date: Jan 12 2026
--- | ---
Rating of: Evaluation of CAE_01/02 Description: Loadcase 01 Rating:
No. | Experiment | Rating | Weight
--- | --- | --- | ---
1 | CAE 1 | 0.6512 | 0.50
2 | CAE 2 | 0.6637 | 0.50
| Total rating of load case 1: | 0.6574 | 1.0

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: CAE 1 Description: Using ISO format 1.0 Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1SENS010000DS0D | 0.6578 | 0.0833
2 | S1SENS020000FO0D | 0.9580 | 0.0833
3 | S1SENS030000ACXA | 0.8222 | 0.0833
4 | S1SENS030000ACYA | 0.3886 | 0.0833
5 | S1SENS030000ACZA | 0.7961 | 0.0833
6 | S1SENS040000FOXA | 0.8771 | 0.0833
7 | S1SENS040000FOYA | 0.4450 | 0.0833
8 | S1SENS040000FOZA | 0.8264 | 0.0833
9 | S1SENS040000MOXB | 0.2631 | 0.0833
10 | S1SENS040000MOYB | 0.6681 | 0.0833
11 | S1SENS040000MOZB | 0.3353 | 0.0833
12 | S1SENS050000DSXC | 0.7765 | 0.0833
| Total rating of experiment 1: | 0.6512 | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 1 of Experiment 1: S1SENS010000DS0D Overall Rating: 0.6578
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.4813 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9613 | 0.8225 | 0.50
Size | 0.7113 | 0.7113 | 0.250
Phase shift | 2.3 | 0.9807 | 0.250
| 0.8343 | 0.50
3 | Combination of 1 and 2 | 0.6578 | -
Parameters: | Evaluation Intervall: | 10.1 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.0887
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.9 - 22.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 2 of Experiment 1: S1SENS020000FO0D Overall Rating: 0.9580
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.9341 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9968 | 0.9841 | 0.50
Size | 0.9595 | 0.9595 | 0.250
Phase shift | -1.1 | 1.0 | 0.250
| 0.9819 | 0.50
3 | Combination of 1 and 2 | 0.9580 | -
Parameters: | Evaluation Intervall: | 9.9 - 169.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 3203.9290
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 3 of Experiment 1: S1SENS030000ACXA Overall Rating: 0.8222
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.7616 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9762 | 0.8873 | 0.50
Size | 0.7891 | 0.7891 | 0.250
Phase shift | 2.5 | 0.9676 | 0.250
| 0.8828 | 0.50
3 | Combination of 1 and 2 | 0.8222 | -
Parameters: | Evaluation Intervall: | 15.7 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 134.1629
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 4 of Experiment 1: S1SENS030000ACYA Overall Rating: 0.3886
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.3268 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.8716 | 0.5150 | 0.50
Size | 0.0940 | 0.0940 | 0.250
Phase shift | -8.4 | 0.6775 | 0.250
| 0.4504 | 0.50
3 | Combination of 1 and 2 | 0.3886 | -
Parameters: | Evaluation Intervall: | 15.3 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 17.7066
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 5 of Experiment 1: S1SENS030000ACZA Overall Rating: 0.7961
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.750 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9294 | 0.6981 | 0.50
Size | 0.9729 | 0.9729 | 0.250
Phase shift | -1.0 | 1.0 | 0.250
| 0.8423 | 0.50
3 | Combination of 1 and 2 | 0.7961 | -
Parameters: | Evaluation Intervall: | 13.5 - 159.8
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 166.750
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 6 of Experiment 1: S1SENS040000FOXA Overall Rating: 0.8771
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.8460 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9881 | 0.9422 | 0.50
Size | 0.7483 | 0.7483 | 0.250
Phase shift | -0.4 | 1.0 | 0.250
| 0.9082 | 0.50
3 | Combination of 1 and 2 | 0.8771 | -
Parameters: | Evaluation Intervall: | 15.8 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 513.8964
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 7 of Experiment 1: S1SENS040000FOYA Overall Rating: 0.4450
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.3180 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9368 | 0.7252 | 0.50
Size | 0.1777 | 0.1777 | 0.250
Phase shift | -7.6 | 0.6599 | 0.250
| 0.5720 | 0.50
3 | Combination of 1 and 2 | 0.4450 | -
Parameters: | Evaluation Intervall: | 18.5 - 178.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 109.9730
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 8 of Experiment 1: S1SENS040000FOZA Overall Rating: 0.8264
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.7609 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9546 | 0.7947 | 0.50
Size | 0.9779 | 0.9779 | 0.250
Phase shift | -1.4 | 1.0 | 0.250
| 0.8918 | 0.50
3 | Combination of 1 and 2 | 0.8264 | -
Parameters: | Evaluation Intervall: | 13.7 - 160.3
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 750.6240
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 9 of Experiment 1: S1SENS040000MOXB Overall Rating: 0.2631
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.1666 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.7624 | 0.2823 | 0.50
Size | 0.0976 | 0.0976 | 0.250
Phase shift | -6.2 | 0.7766 | 0.250
| 0.3597 | 0.50
3 | Combination of 1 and 2 | 0.2631 | -
Parameters: | Evaluation Intervall: | 20.6 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.0472
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.5
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 10 of Experiment 1: S1SENS040000MOYB Overall Rating: 0.6681
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.6428 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.8514 | 0.4621 | 0.50
Size | 0.9221 | 0.9221 | 0.250
Phase shift | 3.3 | 0.9275 | 0.250
| 0.6934 | 0.50
3 | Combination of 1 and 2 | 0.6681 | -
Parameters: | Evaluation Intervall: | 16.4 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 38.8203
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.0
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 11 of Experiment 1: S1SENS040000MOZB Overall Rating: 0.3353
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.3638 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.7058 | 0.2037 | 0.50
Size | 0.4496 | 0.4496 | 0.250
Phase shift | -14.6 | 0.370 | 0.250
| 0.3067 | 0.50
3 | Combination of 1 and 2 | 0.3353 | -
Parameters: | Evaluation Intervall: | 15.9 - 200.0
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 2.8713
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 12 of Experiment 1: S1SENS050000DSXC Overall Rating: 0.7765
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.6431 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9912 | 0.9570 | 0.50
Size | 0.7306 | 0.7306 | 0.250
Phase shift | 1.9 | 0.9951 | 0.250
| 0.9099 | 0.50
3 | Combination of 1 and 2 | 0.7765 | -
Parameters: | Evaluation Intervall: | 14.0 - 194.2
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.0219
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Experiment Report | Date: Jan 12 2026
--- | ---
Report of Experiment: CAE 2 Description: Using XYData format Rating:
No. | Signal | Rating | Weight
--- | --- | --- | ---
1 | S1SENS010000DS0D | 0.7520 | 0.0833
2 | S1SENS020000FO0D | 0.9141 | 0.0833
3 | S1SENS030000ACXA | 0.8020 | 0.0833
4 | S1SENS030000ACYA | 0.2946 | 0.0833
5 | S1SENS030000ACZA | 0.8585 | 0.0833
6 | S1SENS040000FOXA | 0.8906 | 0.0833
7 | S1SENS040000FOYA | 0.5546 | 0.0833
8 | S1SENS040000FOZA | 0.8686 | 0.0833
9 | S1SENS040000MOXB | 0.2624 | 0.0833
10 | S1SENS040000MOYB | 0.7632 | 0.0833
11 | S1SENS040000MOZB | 0.3289 | 0.0833
12 | S1SENS050000DSXC | 0.6747 | 0.0833
| Total rating of experiment 2: | 0.6637 | 1.0

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 1 of Experiment 2: S1SENS010000DS0D Overall Rating: 0.7520
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.5989 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9787 | 0.8985 | 0.50
Size | 0.8235 | 0.8235 | 0.250
Phase shift | 1.5 | 1.0 | 0.250
| 0.9052 | 0.50
3 | Combination of 1 and 2 | 0.7520 | -
Parameters: | Evaluation Intervall: | 10.1 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.0887
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.9 - 22.8
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 2 of Experiment 2: S1SENS020000FO0D Overall Rating: 0.9141
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.8720 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9906 | 0.9540 | 0.50
Size | 0.9166 | 0.9166 | 0.250
Phase shift | 0.6 | 1.0 | 0.250
| 0.9562 | 0.50
3 | Combination of 1 and 2 | 0.9141 | -
Parameters: | Evaluation Intervall: | 9.9 - 169.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 3203.9291
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 3 of Experiment 2: S1SENS030000ACXA Overall Rating: 0.8020
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.7625 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9812 | 0.910 | 0.50
Size | 0.6079 | 0.6079 | 0.250
Phase shift | 3.1 | 0.9379 | 0.250
| 0.8415 | 0.50
3 | Combination of 1 and 2 | 0.8020 | -
Parameters: | Evaluation Intervall: | 15.7 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 134.1629
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 4 of Experiment 2: S1SENS030000ACYA Overall Rating: 0.2946
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.3396 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.7380 | 0.2455 | 0.50
Size | 0.1653 | 0.1653 | 0.250
Phase shift | -15.2 | 0.3424 | 0.250
| 0.2497 | 0.50
3 | Combination of 1 and 2 | 0.2946 | -
Parameters: | Evaluation Intervall: | 15.3 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 17.7066
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 5 of Experiment 2: S1SENS030000ACZA Overall Rating: 0.8585
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.7931 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9755 | 0.8840 | 0.50
Size | 0.9274 | 0.9274 | 0.250
Phase shift | -0.4 | 1.0 | 0.250
| 0.9238 | 0.50
3 | Combination of 1 and 2 | 0.8585 | -
Parameters: | Evaluation Intervall: | 13.5 - 159.8
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 166.750
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 6 of Experiment 2: S1SENS040000FOXA Overall Rating: 0.8906
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.8298 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9846 | 0.9257 | 0.50
Size | 0.9541 | 0.9541 | 0.250
Phase shift | 0.6 | 1.0 | 0.250
| 0.9514 | 0.50
3 | Combination of 1 and 2 | 0.8906 | -
Parameters: | Evaluation Intervall: | 15.8 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 513.8964
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 7 of Experiment 2: S1SENS040000FOYA Overall Rating: 0.5546
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.5361 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9225 | 0.6735 | 0.50
Size | 0.4951 | 0.4951 | 0.250
Phase shift | -11.3 | 0.4501 | 0.250
| 0.5730 | 0.50
3 | Combination of 1 and 2 | 0.5546 | -
Parameters: | Evaluation Intervall: | 18.5 - 178.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 109.9730
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.6 - 19.2
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 8 of Experiment 2: S1SENS040000FOZA Overall Rating: 0.8686
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.8210 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9760 | 0.8861 | 0.50
Size | 0.8927 | 0.8927 | 0.250
Phase shift | -0.8 | 1.0 | 0.250
| 0.9162 | 0.50
3 | Combination of 1 and 2 | 0.8686 | -
Parameters: | Evaluation Intervall: | 13.7 - 160.3
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 750.6240
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.5 - 17.6
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 9 of Experiment 2: S1SENS040000MOXB Overall Rating: 0.2624
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.2812 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.6662 | 0.1610 | 0.50
Size | 0.2722 | 0.2722 | 0.250
Phase shift | -14.0 | 0.3807 | 0.250
| 0.2437 | 0.50
3 | Combination of 1 and 2 | 0.2624 | -
Parameters: | Evaluation Intervall: | 20.6 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 6.0472
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.5
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 10 of Experiment 2: S1SENS040000MOYB Overall Rating: 0.7632
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.7529 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9495 | 0.7743 | 0.50
Size | 0.6126 | 0.6126 | 0.250
Phase shift | -3.2 | 0.9324 | 0.250
| 0.7734 | 0.50
3 | Combination of 1 and 2 | 0.7632 | -
Parameters: | Evaluation Intervall: | 16.4 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 38.8203
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.0
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 11 of Experiment 2: S1SENS040000MOZB Overall Rating: 0.3289
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.3746 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.2568 | 0.0096 | 0.50
Size | 0.8033 | 0.8033 | 0.250
Phase shift | -15.8 | 0.3103 | 0.250
| 0.2832 | 0.50
3 | Combination of 1 and 2 | 0.3289 | -
Parameters: | Evaluation Intervall: | 15.9 - 199.9
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 2.8713
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 22.1
| Rating exponents (shape, size, phase): | 10, 1, 1

Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 2 Report of Signal 12 of Experiment 2: S1SENS050000DSXC Overall Rating: 0.6747
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_02
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.5741 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9856 | 0.9304 | 0.50
Size | 0.8157 | 0.8157 | 0.250
Phase shift | 13.2 | 0.4250 | 0.250
| 0.7754 | 0.50
3 | Combination of 1 and 2 | 0.6747 | -
Parameters: | Evaluation Intervall: | 14.0 - 194.2
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.0219
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.6
| Rating exponents (shape, size, phase): | 10, 1, 1