Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 2 Report of Signal 1 of Experiment 2: S1HEAD0000H3MOX0 Overall Rating: 0.7549
| Average of tests
| annex_a_5_1_cae2
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.7233 |  | 0.40
2 | Phase | 0.5905 |  | 0.20
3 | Magnitude | 0.9668 |  | 0.20
4 | Slope | 0.7703 |  | 0.20
| Overall rating | 0.7549 | Fair | -
Parameters: | Evaluation Intervall: | 7.3 - 30.4
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 180.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 4.6
| Rating exponents (shape, size, phase): | 1, 1, 1
|  | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---