Signal Report | Date: Jan 12 2026
--- | ---
Rating of: Cae 3 Report of Signal 1 of Experiment 3: S1HEAD0000H3FOX0 Overall Rating: 0.8640
| Average of tests
| annex_a_4_3_cae3
| CAE cut and shifted
| Limits Outer corridor
| Limits inner corridor
Method | Name | Rating | Grade | Weight
1 | Corridor | 0.9032 |  | 0.40
2 | Phase | 0.9596 |  | 0.20
3 | Magnitude | 0.9286 |  | 0.20
4 | Slope | 0.6256 |  | 0.20
| Overall rating | 0.8640 | Good | -
Parameters: | Evaluation Intervall: | 4.3 - 90.9
--- | --- | ---
Corridor: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Reference value: | 784.0
| Transition exponent: | 2.0
Cross Correlation: | Limits for phase shift: | 0.0 - 17.3
| Rating exponents (shape, size, phase): | 1, 1, 1
|  | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---