Signal Report | Date: Jan 12 2026
--- | ---
Rating of: CAE 1 Report of Signal 12 of Experiment 1: S1SENS050000DSXC Overall Rating: 0.7765
| test_01 |  | Average of experiments
| test_02 |  | cross-correlation reference
| test_03 |  | cae_01
| test_04 |  | Limits Outer corridor
|  |  | Limits inner corridor
Method | Name | Rating | Weight
1 | Corridor Method | 0.6431 | 0.50
2 |
Correlation Method |  |  |
| Value | Rating | Weight
Cross correlation function | 0.9912 | 0.9570 | 0.50
Size | 0.7306 | 0.7306 | 0.250
Phase shift | 1.9 | 0.9951 | 0.250
| 0.9099 | 0.50
3 | Combination of 1 and 2 | 0.7765 | -
Parameters: | Evaluation Intervall: | 14.0 - 194.2
--- | --- | ---
Method 1: | Max. half width of inner corridor: | 0.050
| Max. half width of outer corridor: | 0.50
| Corridor curve file: |
| Reference value: | 0.0219
| Transition exponent: | 2
Method 2: | Limits for phase shift: | 1.8 - 21.6
| Rating exponents (shape, size, phase): | 10, 1, 1
Previous Signal |  | Up to Experiment | Up to Loadcase | Up to Summary
--- | --- | --- | --- | ---